Für die Nutzung mit einem PC und ZSP via MXDECUP oder MX31ZL:

... die Datei "DSxxxxxx.zsu" in einen beliebigen Ordner kopieren.
Über ZSP dann den Menüpunkt "DECODER" mit "UPDATEN" das Decoderupdateprogramm starten.
Mit "Datei öffnen", in den Ordner die dort gespeicherte ZSU Datei auswählen.

Für die Nutzung mit MXULF:

... die Datei "DSxxxxxx.zsu" auf einen USB-Stick kopieren und wie in der MXULF Anleitung beschrieben, vorgehen.

Für die Nutzun mit MX31ZL via USB-Stick:

... je nach Decodertyp:
> DSxxxxFA.zsu  für alte Fahrdecoder mit 2-stelliger Artikelnummer (MX62, MX63, MX64)
> DSxxxxFN.zsu  für neue Fahrdecoder mit 3-stelliger Artikelnummer (MX620, MX630,...)
> DSxxxxFu.zsu  für Funktions-/Weichendecoder
> DSxxxxSo.zsu  für Sounddecoder

die jeweilige Datei auf einen USB-Stick kopieren.

------------------------------------------------------------------------------------------------------------------

For use with a PC and ZSP via MXDECUP or MX31ZL:

 ... Copy the file "DSxxxxxx.zsu" to a freely chosen folder.
 Start "ZIMO Decoder Update" and click on "File open" in second window. There select the saved .zsu file.

For use with MXULF:

 ... Save the file "DSxxxxxx.zsu" on a USB stick and proceed as described in the MXULF manual.

For usages of MX31ZL with a USB stick:

 save the files to a USB stick and select on MX31ZL the right file for the decoder to update:

 > DSxxxxFA.zsu for old decoders without sound (MX62, MX63, MX64)
 > DSxxxxFN.zsu for new decoders without sound (MX620, MX630,...)
 > DSxxxxFu.zsu for function and accessory decoders
 > DSxxxxSo.zsu for sound decoders

